1. **收集AP信道利用率**

#

sys

\_h

wlan ap-execute ap1 telnet enable

wlan ap-execute ap1 exec-control enable

quit

quit

#

telnet 192.168.1.2

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

sys

\_h

display ar5drv 1 channelbusy

#

display ar5drv 2 channelbusy

#

quit

quit

quit

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

sys

\_h

wlan ap-execute ap2 telnet enable

wlan ap-execute ap2 exec-control enable

quit

quit

#

telnet 192.168.1.3

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

#

sys

\_h

display ar5drv 1 channelbusy

#

display ar5drv 2 channelbusy

#

quit

quit

quit

在CRT上通过记录会话的方式生成TXT文档文档类容为

<WLAN-AC-Shi-MAIN04> telnet 10.20.152.194

Trying 10.20.152.194 ...

Press CTRL+K to abort

Connected to 10.20.152.194 ...

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* Copyright (c) 2004-2012 Hangzhou H3C Tech. Co., Ltd. All rights reserved. \*

\* Without the owner's prior written consent, \*

\* no decompiling or reverse-engineering shall be allowed. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

<WA1208E-GP-H20>sy

System View: return to User View with Ctrl+Z.

[WA1208E-GP-H20]\_H

Now you enter a hidden command view for developer's testing, some commands may

affect operation by wrong use, please carefully use it with our engineer's

direction.

[WA1208E-GP-H20-hidecmd]display ar5drv 1 channelbusy

ChannelBusy information

Ctl Channel: 06 Channel Band: 20M

Record Interval(s): 9

Date/Month/Year: 06/06/2012

Time(h/m/s): CtlBusy(%) TxBusy(%) RxBusy(%)

01 12:00:42 86 0 85

02 12:00:33 89 0 87

03 12:00:24 87 0 86

04 12:00:15 60 0 58

05 12:00:06 88 0 86

06 11:59:57 85 0 84

07 11:59:48 90 0 89

08 11:59:39 91 0 89

09 11:59:30 90 0 88

10 11:59:21 90 0 88

11 11:59:12 89 0 88

12 11:59:02 90 0 89

13 11:58:53 89 0 88

14 11:58:44 54 0 52

15 11:58:35 41 0 39

16 11:58:26 56 0 53

17 11:58:17 37 0 35

18 11:58:08 39 1 36

19 11:57:59 38 0 36

20 11:57:50 23 0 22

[WA1208E-GP-H20-hidecmd]quit

[WA1208E-GP-H20]quit

<WA1208E-GP-H20>quit

The connection was closed by the remote host!

<WLAN-AC-Shi-MAIN04>telnet 10.20.152.195

Trying 10.20.152.195 ...

Press CTRL+K to abort

Connected to 10.20.152.195 ...

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* Copyright (c) 2004-2012 Hangzhou H3C Tech. Co., Ltd. All rights reserved. \*

\* Without the owner's prior written consent, \*

\* no decompiling or reverse-engineering shall be allowed. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

<WA1208E-GP-H20>sy

System View: return to User View with Ctrl+Z.

[WA1208E-GP-H20]\_H

Now you enter a hidden command view for developer's testing, some commands may

affect operation by wrong use, please carefully use it with our engineer's

direction.

[WA1208E-GP-H20-hidecmd]display ar5drv 1 channelbusy

ChannelBusy information

Ctl Channel: 11 Channel Band: 20M

Record Interval(s): 9

Date/Month/Year: 06/06/2012

Time(h/m/s): CtlBusy(%) TxBusy(%) RxBusy(%)

01 12:00:48 26 0 25

02 12:00:39 25 0 23

03 12:00:30 27 0 26

04 12:00:21 41 0 39

05 12:00:12 40 1 37

06 12:00:03 31 0 30

07 11:59:53 28 0 26

08 11:59:44 30 0 28

09 11:59:35 38 0 36

10 11:59:26 41 0 39

11 11:59:17 36 1 33

12 11:59:08 36 0 34

13 11:58:59 36 0 34

14 11:58:50 41 0 39

15 11:58:41 37 0 34

16 11:58:32 45 1 42

17 11:58:23 47 1 45

18 11:58:13 54 0 52

19 11:58:04 58 0 55

20 11:57:55 58 1 55

[WA1208E-GP-H20-hidecmd]quit

[WA1208E-GP-H20]quit

<WA1208E-GP-H20>quit

The connection was closed by the remote host!

<WLAN-AC-Shi-MAIN04>telnet 10.20.152.196

Trying 10.20.152.196 ...

Press CTRL+K to abort

Connected to 10.20.152.196 ...

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* Copyright (c) 2004-2012 Hangzhou H3C Tech. Co., Ltd. All rights reserved. \*

\* Without the owner's prior written consent, \*

\* no decompiling or reverse-engineering shall be allowed. \*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

<WA1208E-GP-H20>sy

System View: return to User View with Ctrl+Z.

[WA1208E-GP-H20]\_H

Now you enter a hidden command view for developer's testing, some commands may

affect operation by wrong use, please carefully use it with our engineer's

direction.

[WA1208E-GP-H20-hidecmd]display ar5drv 1 channelbusy

ChannelBusy information

Ctl Channel: 01 Channel Band: 20M

Record Interval(s): 9

Date/Month/Year: 06/06/2012

Time(h/m/s): CtlBusy(%) TxBusy(%) RxBusy(%)

01 12:00:49 30 0 28

02 12:00:40 29 0 27

03 12:00:31 23 0 21

04 12:00:22 23 0 21

05 12:00:13 21 1 19

06 12:00:03 19 1 17

07 11:59:54 18 1 16

08 11:59:45 21 0 19

09 11:59:36 24 0 22

10 11:59:27 100 100 100

11 11:59:18 22 0 20

12 11:59:09 19 0 18

13 11:59:00 26 0 24

14 11:58:51 19 0 17

15 11:58:42 16 0 14

16 11:58:33 14 0 12

17 11:58:23 20 0 19

18 11:58:14 15 0 14

19 11:58:05 13 0 11

20 11:57:56 12 0 11

[WA1208E-GP-H20-hidecmd]quit

[WA1208E-GP-H20]quit

<WA1208E-GP-H20>quit

The connection was closed by the remote host!

<WLAN-AC-Shi-MAIN04>telnet 10.20.152.197

Trying 10.20.152.197 ...

Press CTRL+K to abort

找到AP对应地址，根据时间记录信道利用率即可。